


	`
	DESCRIPTION
	MAXIMUM
SCORE
	ACTUAL
SCORE
	REMARKS

	1.
(a)
(b)

(c)

(d)
	PRESENTATION
Work well pressed(½) and folded (½)
Label (½) firmly fixed (½) without concealing details(½) and on a single fabric(½)
Pins/ needles (½) and unnecessary tacking threads(½) and hanging threads (½) removed
Made up for the left half(1)
	
1

2

1½
1
	
	

	
	Sub- total
	5½
	
	

	2. 
(a)
(b)

(c)

(d)

(e)

(f)

(g)
(h)
	CUTIING OUT
All ten pieces cut out (10 x½)
Smooth cutting of the skirt at CF (1) on straight grain (1) within 2 mm
Smooth cutting of the skirt at CB (1) on straight grain (1) within 2 mm
Lower edge of frill (1) and lower edge of skirt (1) smoothly cut
Waistband CB smoothly cut (½x3) on straight grain (½x3)
Waistband CF smoothly cut (½x3) on straight grain (½x3)
Smooth cutting of yoke (1) and on a straight grain (1)
Smooth cutting of frill CF (½) on grain (½)



	
5

2

2

2

3
3


2
1
	
	

	
	Sub- total
	20
	
	

	3
(a)
(b)
(c)

(d)

(e)
(f)

	DART
Straight stitchery (1) tapering to a point (½)
Threads ends well fastened at the point (1)
Correct length of the dart 8cm to within 2 mm (7.8 cm-8.2 cm (1) 
Correct width of the dart 1 cm to within 2 mm (0.8 cm -1.2 cm)  (1)
Dart pressed (½) towards C.B(½)
Flatness of dart onR.S (½) and W.S (½) (NO pockets formed)

	
1½
1

1

1
1

1
	
	

	
	Sub- total
	6½
	
	


HOME SCIENCE PAPER 2 MARKING SCHEME

	`
	DESCRIPTION
	MAXIMUM
SCORE
	 ACTUAL 
SCORE
	REMARKS

	4.

(a)
(b)
(c)
(d)

(e)

(f)

(g)

	YOKE
(If not overlaid seam award zero)
Front yoke folded on seamline (1)
Placed on fitting line of lower skirt front (1)
Notches matching (1)
Straight stitchery (1) at the edge of the fold to within 2 mm (1)
Overlaid seam turning facing up towards waist (½) and even (½)
Seam trimmed 1 cm from fitting line to within 2 mm (08 cm-1.2 cm) )
Flatness of yoke on R. S  (1)
	

1
1
1

2

1

1
1

	
	

	
	                                                       Sub- total
	8
	
	

	5. 

(a)
(b)

	NEATING OF THE OVERLAID SEAM
(if not loop stitches award zero)
Loop stiches evenly spaced (1) and even in length (1).
Seam halfway neatened (1) and stitches securely fastened on (½) and off(½)

	

2

2
	
	

	
	                                                        Sub- total
	4
	
	

	6
(a)

(b)
(c)
(d)
(e)


(f)

	FRILL
Two rows of gathering stitches above (1) and below (1) the stitching line
Gathers evenly distributed (no pleats or clusters) (2)
Frill attached with straight stitchery (2)
Notches matching (1)
Correct size of seam allowance (1) 1.5 cm to within 2 mm(1.3 cm-1.7 cm) and evenness (1) of the seam allowance
Seam allowance pressed flat () facing upward (½)


	

2
2
2
1


2
1

	
	

	
	 Sub- total
	10
	
	

	7.

(a)

(b)
(c)
(d)

(e)


	OPEN SEAM
(If not open seam award zero)
Seam jointed with straight stitchery (1½) and well secured at the yoke or hemline band (½)
Seam appropriately neatened (1x 2)
Evenness of seam allowance (½ x2)
Correct width 1 cm to within 2 mm on either side
 (0.8 cm -1.2 cm) (½ x 2)
Seams turning folded (½) and flat(½) at he waistband

	


2
2
1

1
1

	
	

	
	 Sub- total
	7
	
	



	`
	DESCRIPTION
	MAXIMUM
SCORE
	ACTUAL
SCORE
	REMARKS

	8.
(a)

(b)

(c)
(d)

(e)

(f)
(g)
(h)
(i)

(j)
(k)
	WAISTBAND
Waistband joined with straight stitchery (mark by impression) (2)
Seam trimmed (1) snipped (1½) with sharp corners (½x3)
Waistband well knife edged (½x2)
Back waistband extension 3 cm to within 5 mm (2.5cm- 3.5 m) (1)
Waistband correctly attached with straight stitchery (1x 2) and trimmed (½ x2)
Raw edges of waistband well tucked under (1 x2)
Flatness of waistband on R.S (1) and W.S (1)
Evenness of the waistband R.S  (1)
Correct width of waistband 3 cm to within 3 mm (2.7 cm-3.3 cm) (1)
Waistband CF flash with C.F of oke (½) and C.B of skirt back ( ½)
Tacking stitches even (½) and straight (½), firm (½) made using single tread (½)

	

2

4

1
1

3
2
2
1

1
1

2

	
	

	
	                                                       Sub- total
	20
	
	

	9. 

(a)

(b)

(c)

(d)

(e)

(f)
(f)


	WORKED BUTTON HOLE (ONE ROUND END)
(If not buttonhole award zero from C to F).
Correct position(½) and size (½) of buttonhole (mark by impression)
Buttonhole cut straight (½) and worked with single thread(½)
Buttonhole worked with even (1) correct tension (1) and well distributed (1) buttonhole stitches
Round end worked with even (1) and well distributed (1) overcasting stitches
Square end completed with a bar (½) worked with even buttonhole stitches (½)
Raw edges (½x 2) concealed by thebuttonhole stitches on the right side.


	


1
1

3

2

2

1
	
	

	
	 Sub- total
	9
	
	

	
	TOTAL
	90
	
	

	
	                                                       Actual score
                           FINAL MARK=            2
	
	
	


























GIRL'SSKIRT
Apatternofagirl'sskirtisprovided.Youareadvisedtostudythesketches,instructionsandlayoutcarefullybeforeyoubeginthetest.
MATERIALSPROVIDED
1.PatternPieces
A— Skirtback
B—Yoke(front)
C—Lowerskirt(front)
	D—Frontwaistband
E—Backwaistband
F—Frill

2.Plainlightweightcottonfabric56cmlongby90cmwide.
3Sewingthreadtomatchthefabric.
4Onelargeenvelope.

THETEST
Usingthematerialsprovided,cutoutandmakethelefthalfofthegirl'sskirttoshowthefollowingprocesses:
a) Cuttingout.(18marks)
b) Makingofthedartatthebackskirt.(61/2marks)
c) Joiningoftheyokefronttothelowerskirtfrontusinganoverlaidseam.Donottrim.Neatenhalftheseamusingloopstitches.(12marks)
d) Attachingofthefrilltothelowerskirtfrontusingaplainseam.Leavethegatheringstitchesanddonottrimtheseamallowance.(11marks)
e) Makingoftheskirtsideseamfromtheyoketothehemlineusinganopenseam.(7marks)
f) Attachingofthefrontandbackwaistbandsandholdingtheminplaceusingtackingstitches.(20marks)

g) Makingoftheworkedbuttonhole.(12marks)
h) OMITThemanagementoftheskirthem.
i) Overallpresentation.(61/2marks)
Attheendoftheexamination,firmlysewontoyourwork,onasinglefabric,alabelbearingyourname and index number. Remove the needle, pins and loose threads from your work. Fold yourworkneatlyandplaceitintheenvelopeprovided.Donotputscrapsoffabricintheenvelope.Donotsealtheenvelope.
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