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INSTRUCTIONS TO CANDIDATES
a) This paper consists of 3 printed pages.
b) Candidates should check the question paper to ascertain that all the pages are printed as indicated and that no questions are missing.
c) Candidates MUST use machine stitches appropriately in the construction of the garment.
Hand stitches used instead of machine stitches will not be marked.
d) Hand stitches will only be allowed for the making of loop, worked buttonhole tacking stitches.


Candidates should check the question paper to ensure that both
Pages are printed as indicated and no questions are missing.

                    	Turn over
GIRL'S SKIRT
A pattern of a girl's skirt is provided. You are advised to study the sketches, instructions and layout  carefully before you begin the test.
MATERIALS PROVIDED
1. Pattern Pieces
A — Skirt back
B — Yoke (front)
C — Lower skirt (front)
               	D — Front waistband
E — Back waistband
F — Frill

2.Plain lightweight cotton fabric 56 cm long by 90 cm wide.
 3 Sewing thread to match the fabric.
4 One large envelope.

THE TEST
Using the materials provided, cut out and make the left half of the girl's skirt to show the following processes:
a) Cutting out. (18 marks)
b) Making of the dart at the back skirt. (61/2 marks)
c) Joining of the yoke front to the lower skirt front using an overlaid seam. Neaten half the seam using loop stitches. (12 marks)
d) Attaching of the frill to the lower skirt front using a plain seam. Leave the gathering stitches and do not trim the seam allowance. (11 marks)
e) Making of the skirt side seam from the yoke to the hemline using an open seam. (7 marks)
f) Attaching of the front and back waistbands and holding them in place using even tacking stitches. (20 marks)
g) Making of the worked buttonhole. (12 marks)
h) OMIT The management of the skirt hem.
i) Overall presentation. (61/2 marks)

At the end of the examination, firmly sew onto your work, on a single fabric, a label bearing your name and index number. Remove needles, pins and loose threads from your work. Fold your work neatly and place it in the envelope provided. Do not put scraps of fabric in the envelope. Do not seal the envelope.
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